Distance Sensor – Laser so it doesn’t measure the table

Encoder Cable – To make the encoder actually work

Higher Power Motor – To increase response speed

AA Battery Case – To power the motors

Jumper Cables – To prototype

Logic Level Converter – Distance Sensor is 3.3V